# APPROVED MATERIALS LIST

Contractor must select products that meet the following use and specifications. Products used that do not meet specifications and use outlined in this table will be considered a default of Contract due to non-compliance. Estimated quantity is annually per Rest Area.

|  |  |  |  |
| --- | --- | --- | --- |
| **MATERIAL** | **TYPICAL USE** | **MATERIAL SPECIFICATIONS** | **ESTIMATED QUANTITY**  **ANNUALLY** |
| **Toilet Paper** | Jumbo Junior Toilet Paper Containers | Toilet tissue dispenser roll, single-ply white, non-perforated, 3 3/4” wide, 3” core, 2000’/roll, 12/rolls per case | 1200 cases |
|  | Regular Toilet Paper Containers | Toilet Tissue Rolls, bleached, 2 ply wrapped 4 ½” x 4 ½” 100 sheets/roll, 96 rolls/case | 1800 cases |
| **Scented Urinal Pads** | Urinal |  | 48 |
| **Liquid Hand Soap** | All manual hand soap dispensers | Soap must be mild, liquid and remain viscous at temperatures 40 degrees F or higher. Must be designed for hand soap dispensers. Soaps that clog dispensers will not be allowed. | 120 Gallons |
| **Plastic Bag Barrel Liners (55gal)** | All large trash barrels | 55 gal. Capacity, minimum size 36” x 60”, mil thickness .16 | 2600 Bags |
| **Plastic Bag Barrel Liners (33gal)** | Trash Cans | 33 gal. Capacity, minimum size 33” x 40”, mil thickness .43 | 1000 Bags |
| **Sanitary Napkin Disposal Bag** | Sanitary Napkin Receptacles | Approved dispenser liner that fits properly | 6000 Bags |
| **Glass Cleaner** | All glass and mirrored surfaces | Liquid spray, formula designed or cleaning glass and mirrors, non-abrasive | 60 Gallons |
| **Toilet Bowl and Urinal Cleaner** | To disinfect inside of urinals, bowls, flushing cavities | E.P.A. Approved HCI acid base bowl cleaner (10% maximum HCL) | 250 Gallons |
| **Rotary Floor Machine – Liquid Cleaner** | To clean tile floors once per month | E.P.A. Approved 20-36% phosphoric acid base cleaner | 10 Gallons |
| **Liquid Detergent- Synthetic**  **Disinfectant** | To clean, disinfect tile floor, walls, partitions, sink tops, sinks, outside of toilets, urinals, toilet seats, and sanitary napkin  disposal containers | E.P.A. Registered disinfectant, detergent shall be quaternary ammonium compounds | 40 Gallons |
| **MATERIAL *(Con’t.)*** | **TYPICAL USE** | **MATERIAL SPECIFICATIONS** | **ESTIMATED QUANTITY** |
| **Stainless Steel Cleaner** | To clean metal surfaces | Safe for metals, non-scouring product | 3 Gallons |
| **De-icing Chemical** | To use on sidewalks and entrances for ice removal | Calcium Chloride or product approved (NO ROCK SALT) | 4000 Pounds |
| **Marker/Vandal Remover** | To remove crayon, pen, marker, ink, paint and pencil marks | Must be safe for use on hard surfaces such as painted walls, brick, tile and laminates | 10 – 16 oz Cans |
| **Latex Gloves** | To be used when cleaning facility | Quality disposable gloves (Latex) | 24 Pair |
| **Personal Eye Wash** | To be readily available and accessible when using cleaning products | 23-oz. Polyethylene eye wash bottle | 2 Bottles |
| **Wet Floor Signs** | To be placed in areas being cleaned when needed | Approved plastic yellow folding signs | 3 Signs |
| **Cotton Mops** | To mop tile flooring | Cotton blend, banded loop (min. 2) | 24 |
| **Mop Handle** | To be used with Cotton Mops | Plastic grips or speed change heads | 3 |
| **Scrub Pads** | To be used to manually scrub areas not easily accessible by Rotary Floor Machine | Swivel head must fit on standard threaded wood handle with bristle made of DuPont “Tynex A” | 1 |
| **Handles** | To hold Scrub Pad | Standard thread, wood | 1 |
| **Mop Bucket & Wringer** | To hold solution and Drain Mop | Bucket must be on rollers, wringer must match bucket and mop size | 1 |
| **Floor Squeegees** | To push excess liquid into floor drains | 24” minimum width, rubber tipped | 5 |
| **Broom** | To sweep dirt and debris from floor | Heavy duty push broom, 24” minimum width, for interior hard floor surfaces | 5 |
| **Window Squeegees and Extension** | To clean windows | Squeegee designed for window washing with extension as needed | 5 |
| **Toilet Bowl Mop** | To clean inside toilet bowl and urinals | Cotton or synthetic mop – no brushes | 24 |
| **Spray Bottles** | To hold various cleaning supplies | Clean plastics, trigger style bottles | 10 |
| **Sponges, Cloths** | To clean surfaces | Cotton cloths, absorbent sponges | 10 |
| **Air Blower** | To dry floors | 1 HP motor, minimum 4,000cfm | 1 |
| **Wet-Dry Vacuum** | To clean floors, mats, air vents, filters, ledges, etc. | Minimum 6.0 Peak Hp, capacity 16 gallons, w/appropriate attachments | 1 |
| **MATERIAL *(Con’t.)*** | **TYPICAL USE** | **MATERIAL SPECIFICATIONS** | **ESTIMATED QUANTITY** |
| **Rotary Floor Machine** | To scrub quarry tile floors | 175 RPM speed with 15” Brush Spread, must be run on wet floor | 1 |
| **Rotary Brush Head** | To scrub quarry tile floor | “Zim Grit” 15” diameter solid wood back, green color with 40 gauge Tynex nylon filament – must fit above Rotary Floor Machine | 1 |
| **Portable Pump-up Sprayer** | To wash walls and partitions | Portable, 3 Gallon capacity, plastic tank with 18” chemical resistant hose with wand, adjustable spray tip, viton seals | 1 |
| **Multipurpose, Telescoping Ladder** | To use when accessing certain varying heights | Step ladder height 6 to 9 feet,  ANSI Type 1A | 1 |
| **Florescent Bulbs** | To replace lighting | 40 Watt | 24 |
| **Toilet Plunger** | To unclog toilets | Standard | 1 |
| **Drain Snake** | To unclog drains | Standard | 1 |
| **Aerosol Gum Remover** | Remove gum from floors | Aerosol cans | 12 |
| **Shredded Mulch Bark** | To be placed around trees & plant beds | No wood chips or foreign objects (i.e., rocks, nails, etc.) | 10 cubic yards approximately |
| **Snow Blower** | To remove snow on walks/plaza areas | Minimum 7 horsepower, 2 stage blower | 1 |